**ClearFire®-CE**

**Fully Condensing**

* Fully condensing high-mass firetube boiler
* Compact footprint
* 750 to 2,000 MBTU
* Standard less than 20 ppm NOx
* Variable flow capable with no minimum flow requirement
* Standard dual-return connections

The ClearFire®-CE (CFC-E) is a compact, high-mass, fully condensing hydronic boiler, capable of variable-flow pumping, allowing for maximum operating efficiency in a variety of system applications.