**Low Emissions Performance**

* Steam and hot water
* 75 to 250 HP
* Available to <9 ppm NOx, ultra-low CO
* Natural gas or propane fuel
* Premix burner technology

The Model FLXPM Flextube boiler achieves best-in-class combustion performance with low emissions. Premix burner technology enables the boiler to attain <20 ppm NOx without FGR and <10 CO as standard on natural gas. The modulating burner control automatically adjusts the air/gas mixture for maximum efficiency and optimum turndown.